For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the instrument panel storage compartment. Refer to Instrument Panel Storage Compartment Replacement .
3. Remove the footwell upper cover.
4. Remove the motor and the seal from the heater/air distribution case by gently pulling the motor straight down and out.
5. Remove the screws that secure the motor to the heater/air distributor case.

### Installation Procedure

1. Install the blower motor and the seal with the shock mount pads in the heater/air distributor case. Hold the blower motor in position.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the screws to secure the blower motor to the heater/air distributor case.

Tighten
Tighten the blower motor-to-heater/air distributor case screws to 6 N·m (53 lb in).

3. Connect the blower motor electrical connector.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
5. Confirm that the blower motor operates properly.
6. Install the footwell upper cover.
7. Install the instrument panel storage compartment. Refer to Instrument Panel Storage Compartment Replacement .