For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement.
2. Remove the screws and driver information bezel.
3. Remove the screws and the digital clock.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the digital clock with the screws and tighten to 2 N·m (18 lb in).
2. Install the driver information bezel with the screws.
3. Install the I/P center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement.