For 1990-2009 cars

### Removal Procedure

1. Remove the sunroof window. Refer to Sunroof Window Replacement .
2. Remove the sunroof drain gutter. Refer to Sunroof Water Gutter Replacement .
3. Slide the sunshade forward to the closed position.
4. Push the spring retainer clips on the right side of the sunshade inward to disengage them from the track using an upward lifting motion.
5. Remove the sunshade from the sunroof module.

### Installation Procedure

1. Engage one side of the sunshade by positioning the spring clips into the track.
2. Push the spring retainer clips inward on the opposite side of the sunshade to engage them into the track.
3. Slide the sunshade back and forth to ensure proper operation.
4. Slide the sunshade to the half closed position.
5. Install the rear drain gutter. Refer to Sunroof Water Gutter Replacement .
6. Install the sunroof window. Refer to Sunroof Window Replacement .