For 1990-2009 cars

Connector 1: | Fuel Door Lock Actuator
Connector 2: | Door Latch - Driver
Connector 3: | Door Latch - Driver (w/Dead Locking)
Connector 4: | Door Latch - Left Rear
Connector 5: | Door Latch - Passenger
Connector 6: | Door Latch - Right Rear
Connector 7: | Door Lock Switch - Driver
Connector 8: | Hood Open Switch
Connector 9: | Inclination Sensor
Connector 10: | Intrusion Sensor
Connector 11: | Liftgate Actuator
Connector 12: | Liftgate Ajar
Connector 13: | Liftgate Glass
Connector 14: | Liftgate Key Cylinder
Connector 15: | Power Sounder
Connector 16: | Remote Control Door Lock Receiver
Connector 17: | Theft Deterent Control Module
Connector 18: | XBCM X1
Connector 19: | XBCM X2

### Fuel Door Lock Actuator

#### Connector Part Information

- OEM: PED 15332130
- Service: N/A
- Description: 2-Way M GT 150 Unsealed

#### Fuel Door Actuator

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | -- | Door Lock Actuator Lock Control
2 | BN | -- | Door Lock Actuator Unlock Control

### Door Latch - Driver

#### Connector Part Information

- OEM: TYCO 6-1355688-1
- Service: N/A
- Description: 10-Way F M/T Sealed

#### Door Latch - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY/BK | -- | Driver Door Ajar Switch Signal
2 | BN | -- | Driver Door Open Switch Signal
3 | BK | -- | Ground
4 | PU | -- | Door Lock Key Switch Unlock Signal
5 | -- | -- | Not Used
6 | BN | -- | Driver Door Double Lock Actuator Lock Control
7 | BN | -- | Door Lock Actuator Unlock Control
8 | GY | -- | Door Lock Actuator Lock Control
9 | L-GN | -- | Door Lock Key Switch Lock Signal
10 | -- | -- | Not Used

### Door Latch - Driver (w/Dead Locking)

#### Connector Part Information

- OEM: TYCO 6-1355688-1
- Service: N/A
- Description: 10-Way F M/T Sealed

#### Door Latch - Driver (w/Dead Locking)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Driver Door Double Lock Actuator Lock Signal
2 | BN | -- | Door Lock Actuator Unlock Control
3 | GY | -- | Door Lock Actuator Lock Control
4 | L-GN | -- | Door Lock Key Switch Signal
5 | -- | -- | Not Used
6 | BN/WH | -- | Driver Door Ajar Switch Signal
7 | -- | -- | Not Used
8 | BK | -- | Ground
9 | PU | -- | Door Lock Key Switch Unlock Signal
10 | -- | -- | Not Used

### Door Latch - Left Rear

#### Connector Part Information

- OEM: TYCO 6-1355683-1
- Service: N/A
- Description: 6-Way F M/T Sealed

#### Door Latch - Left Rear

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Door Double Lock Actuator Lock
2 | BN | -- | Door Lock Actuator Unlock Control
3 | GY | -- | Door Lock Actuator Lock Control
4 | BN/WH | -- | Left Rear Door Ajar Switch Signal
5 | -- | -- | Not Used
6 | BK | -- | Ground

### Door Latch - Passenger

#### Connector Part Information

- OEM: TYCO 6-1355688-1
- Service: N/A
- Description: 10-Way F M/T Sealed

#### Door Latch - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN/WH | -- | Passenger Door Ajar Switch Signal
2 | -- | -- | Not Used
3 | BK | -- | Ground
4 | PU | -- | Door Lock Key Switch Unlock Signal
5 | -- | -- | Not Used
6 | BN | -- | Passenger Door Double Lock Actuator Lock Control
7 | BN | -- | Door Lock Actuator Unlock Control
8 | GY | -- | Door Lock Actuator Lock Control
9 | L-GN | -- | Door Lock Key Switch Lock Signal
10 | -- | -- | Not Used

### Door Latch - Right Rear

#### Connector Part Information

- OEM: TYCO 6-1355683-1
- Service: N/A
- Description: 6-Way F M/T Sealed

#### Door Latch - Right Rear

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Door Double Lock Actuator Lock
2 | BN | -- | Door Lock Actuator Unlock Control
3 | GY | -- | Door Lock Actuator Lock Control
4 | BN/WH | -- | Right Rear Door Ajar Switch Signal
5 | -- | -- | Not Used
6 | BK | -- | Ground

### Door Lock Switch - Driver

#### Connector Part Information

- OEM: PED 13513469
- Service: N/A
- Description: 4-Way F 064 Unsealed

#### Door Lock Switch - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG/BK | -- | Lock Signal
2 | BK | -- | Ground
3 | OG/BK | -- | Unlock Signal
4 | -- | -- | Not Used

### Hood Open Switch

#### Connector Part Information

- OEM: PED 15326808
- Service: N/A
- Description: 3-Way F Sealed

#### Hood Open Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | -- | Hood Closed S/W Signal
2 | -- | -- | Not Used
3 | BK | -- | Ground

### Inclination Sensor

#### Connector Part Information

- OEM: PED 15324229
- Service: N/A
- Description: 4-Way F Timer Micro I Unsealed (BK)

#### Inclination Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | -- | -- | Not Used
3 | L-BU | -- | Incline Sensor Alarm On Signal
4 | D-GN | -- | Alarm Armed Signal

### Intrusion Sensor

#### Connector Part Information

- OEM: TYCO 368500-1
- Service: N/A
- Description: 3-Way F 070 Unsealed

#### Intrusion Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GN | -- | Alarm Armed Signal
2 | PU | -- | Intrusion Sensor Alarm ON Signal
3 | RD/WH | -- | Battery Positive Voltage

### Liftgate Actuator

#### Connector Part Information

- OEM: MG 620490
- Service: N/A
- Description: 2-Way M MN-AL Unsealed

#### Liftgate Actuator

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Door Lock Actuator Unlock Control
2 | GY | -- | Door Lock Actuator Lock Control

### Liftgate Ajar

#### Connector Part Information

- OEM: MG 651201-4
- Service: N/A
- Description: 2-Way F 090III Unsealed (GY)

#### Liftgate Ajar

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | -- | Liftgate Ajar Switch Signal (1)
2 | BK | -- | Ground

### Liftgate Glass

#### Connector Part Information

- OEM: TYCO 936227-1
- Service: N/A
- Description: 4-Way F 090III Unsealed

#### Liftgate Glass

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Ground
2 | PK/BK | -- | Liftgate Ajar SW Signal 1
3 | BN | -- | Lift Glass/Trunk MTR Release Control
4 | BK | -- | Ground

### Liftgate Key Cylinder

#### Connector Part Information

- OEM: TYCO 368538-1
- Service: N/A
- Description: 2-Way F 070 Unsealed

#### Liftgate Key Cylinder

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Trunk Key Switch Signal
2 | BK | -- | Ground

### Power Sounder

#### Connector Part Information

- OEM: TYCO 1-967640-1
- Service: N/A
- Description: 4-Way F MQs Sealed

#### Power Sounder

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Run/Crank Ignition 1 Voltage
2 | RD/WH | -- | Battery Positive Voltage
3 | PK | -- | Power Sounder Enable Signal
4 | BK | -- | Ground

### Remote Control Door Lock Receiver

#### Connector Part Information

- OEM: JAEIL AG5-4S-S3C1
- Service: N/A
- Description: 4-Way F AG5 Unsealed

#### Remote Control Door Lock Receiver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | GN | -- | Low Speed GMLAN Serial Data
3 | -- | -- | Not Used
4 | BK | -- | Ground

### Theft Deterent Control Module

#### Connector Part Information

- OEM: TYCO 368502-1
- Service: N/A
- Description: 6-Way F 070 Unsealed

#### Theft Deterent Control Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY/BK | -- | Courtesy Lamp Relay Control
2 | BK | -- | Ground
3 | D-GN | -- | Low Speed GMLAN Serial Data
4 | BK | -- | Ground
5 | D-BU | -- | Accessory Wakeup Serial Data
6 | RD/WH | -- | Battery Positive Voltage

### XBCM X1

#### Connector Part Information

- OEM: PED 12110088
- Service: N/A
- Description: 24-Way F Metri-pack Unsealed

#### XBCM X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | -- | -- | Not Used
A2 | RD/WH | -- | Battery Positive Voltage
A3 | D-GN | -- | Low Speed GMLAN Serial Data
A4-A6 | -- | -- | Not Used
A7 | BK | -- | Ground
A8-A12 | -- | -- | Not Used
B1 | -- | -- | Not Used
B2 | PK | -- | Run/Crank Ignition Voltage
B3 | -- | -- | Not Used
B4 | BN/BK | -- | Power Sounder Enable Signal
B5-B6 | -- | -- | Not Used
B7 | BK | -- | Ground
B8 | -- | -- | Not Used
B9 | YE | -- | Security Indicator Control
B10 | L-BU | -- | Inclination Sensor Alarm On Signal
B11 | -- | -- | Not Used
B12 | WH | -- | Power Sounder Enable Signal

### XBCM X2

#### Connector Part Information

- OEM: PED 15357040
- Service: N/A
- Description: 8-Way F Metri-Pack 280 Unsealed (GN)

#### XBCM X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | RD/WH | -- | Battery Positive Voltage
C | RD/WH | -- | Battery Positive Voltage
D | BN | -- | Door Double Actuator Look Control
E | -- | -- | Not Used
F | BN | -- | Ground
G-H | -- | -- | Not Used