For 1990-2009 cars

### Removal Procedure

1. Remove the I/P center trim panel.
2. Remove the I/P accessory bezel.
3. Remove the I/P stow tray.
4. Remove the front radio speaker and grille.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the front radio speaker with the screws.

Tighten
Tighten the door speaker screws to 2 N·m (18 lb in).

2. Install the front radio speaker grille.
3. Install the I/P Stow tray with the screws.

Tighten
Tighten the I/P stow tray screws to 2 N·m (18 lb in).

4. Install the I/P accessory bezel with the screws.

Tighten
Tighten the I/P accessory bezel screws to 2 N·m (18 lb in).