For 1990-2009 cars

#### Liftgate Module

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine OFF/Liftgate Closed
Battery Voltage Signal 2 | Data | Voltage | Varies
Hall Sensor Feed Status | Data | No Output/Short to Ground | No Output
Liftgate Handle Switch Status | Data | Active/Inactive | Inactive
Liftgate Ajar Switch | Data | Active/Inactive | Inactive
Object Detection Sensor Status | Data | Voltage | 3.33 V
Object Sensor Supply Voltage | Data | Active/Inactive | Active
LGM Clutch Actuator Command | Data | Active/Inactive | Inactive
LGM Latch Motor Cinch Command | Data | Active/Inactive | Inactive
LGM Latch Pawl Switch | Data | Active/Inactive | Inactive
LGM Latch Ratchet Switch | Data | Active/Inactive | Inactive
LGM Latch Motor Release Command | Data | Active/Inactive | Inactive
LGM Latch Sector Switch | Data | Active/Inactive | Inactive
LGM Motor Closed Command | Data | Active/Inactive | Inactive
LGM Motor Open Command | Data | Active/Inactive | Inactive
LGM Open/Close Position Learned | Data | Yes/No | Yes
LGM Full Open Switch | Data | Active/Inactive | Inactive