For 1990-2009 cars

## Rear Door Frame Applique Replacement C100/Long Body

### Removal Procedure

1. Reposition the weatherstrip in order to access the screws.
2. Remove the screws and the rear side door window frame applique.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the screws and the rear side door window frame applique and tighten to 1.3 N·m (12 lb in).
2. Install the weatherstrip to its original position.

## Rear Door Frame Applique Replacement C105/Short Body

### Removal Procedure

1. Open the rear door.
2. Remove the rear door upper trim panel.
3. Remove the rear door frame applique screws.
4. Remove the rear door frame applique.

### Installation Procedure

1. Install the rear door frame applique.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the screws to the rear door frame applique and tighten to 1.3 N·m (12 lb in).
3. Install the rear door upper trim panel.