For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the screws and the rear console box.
3. Remove the rear console cover and disconnect the connector.
4. Remove the screws and heating mat switch.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the heating mat switch with the screws.

Tighten
Tighten the heating mat switch screws to 2 N·m (18 lb in).

2. Connect the connector and install the rear console cover.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the rear console box with the screws.

Tighten
Tighten the rear console deposit box screws to 2 N·m (18 lb in).

4. Connect the negative battery cable.