For 1990-2009 cars

## Body Side Window Rear Garnish Molding Replacement C 100/Long Body

### Removal Procedure

1. Remove the rear seat lower belts. Refer to Seat Belt Retractor Replacement - No. 1 Rear or Seat Belt Retractor Replacement - No. 2 Rear .
2. Remove the screws and the quarter window garnish molding.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the quarter window garnish molding with the screws.

Tighten
Tighten the quarter window garnish molding screws to 2 N·m (18 lb in).

2. Install the rear seat lower belts. Refer to Seat Belt Retractor Replacement - No. 1 Rear or Seat Belt Retractor Replacement - No. 2 Rear .

## Body Side Window Rear Garnish Molding Replacement C 105/Short Body

### Removal Procedure

1. Remove the rear seat lower belts. Refer to Seat Belt Retractor Replacement - No. 1 Rear or Seat Belt Retractor Replacement - No. 2 Rear .
2. Remove the screws and the quarter window garnish molding.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the quarter window garnish molding with the screws.

Tighten
Tighten the quarter window garnish molding screws to 2 N·m (18 lb in).

2. Install the rear seat lower belts. Refer to Seat Belt Retractor Replacement - No. 1 Rear or Seat Belt Retractor Replacement - No. 2 Rear .