For 1990-2009 cars

### Removal Procedure

1. Turn the ignition to Off.
2. Remove the engine coolant reservoir. Refer to Radiator Surge Tank Replacement .
3. Remove the underhood fuse center.
4. Clean the EBCM to brake pressure modulator valve (BMPV) mounting area.
5. Disconnect the electronic brake control module (EBCM) connector (1).
6. Remove the EBCM attaching screws (1).
7. Remove the EBCM.

### Installation Procedure

1. Clean the sealing surface of the BPMV.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the EBCM to the BPMV assembly. Secure with screws (1), tighten screws in a criss-cross pattern.

Tighten
Tighten the nuts to 3 N·m (27 lb in).

3. Connect the electronic brake control module (EBCM) connector (2).
4. Install the underhood fuse center.
5. Install the engine coolant reservoir. Refer to Radiator Surge Tank Replacement .
6. Perform the Diagnostic System Check - Vehicle . Refer to Control Module References for programming and setup information.