For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Disconnect the brake line from the brake hose support bracket on the wheel housing on each side of the vehicle.
3. Remove the retainer.
4. Remove the brake hose from the wheel housing bracket.
5. Remove the brake hose from the clip.
6. Remove the brake hose from the brake caliper.
7. Remove the brake hose from the retainers and retaining bracket from the strut.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the new brake hose to the caliper with the new seal rings and the bolt.

Tighten
Tighten the front brake hose-to-caliper bolt to 40 N·m (30 lb ft).

2. Install the brake hose and clip to the retaining bracket. Connect the brake hose to brake pipe line.

Tighten
Tighten the brake line fittings to 16 N·m (12 lb ft).

3. Install the brake hose to the clips.
4. Lower the vehicle.
5. Bleed the brake system. Refer to Hydraulic Brake System Bleeding .
6. Check the brake system for leaks.