For 1990-2009 cars

### Removal Procedure

Note: Left - Hand Drive Shown, Right - Hand Drive Similar.

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Open the instrument panel compartment.
3. Remove the instrument panel compartment lamp.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the instrument panel compartment lamp.
3. Close the instrument panel compartment.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.