For 1990-2009 cars

### Removal Procedure

1. Remove the screws (1).
2. Remove the lower splash guard to rocker panel molding retainer.
3. Remove the splash guard (2).

### Installation Procedure

1. Install the splash guard (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the screws (1).

Tighten
1.5 N·m (13 lb in)

3. Install the lower splash guard to rocker panel molding retainer.