For 1990-2009 cars

## Driver Information Center Replacement C100/Long Body

### Removal Procedure

1. Remove the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement.
2. Remove the screws and the driver information bezel.
3. Remove the screws and the driver information center.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the driver information center with the screws and tighten to 2 N·m (18 lb in).
2. Install the driver information bezel with the screws and tighten to 2 N·m (18 lb in).
3. Install the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement.

## Driver Information Center Replacement C105/Short Body

### Removal Procedure

Note: Left-Hand Drive Shown, Right-Hand Drive Similar.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement.
3. Remove the radio. Refer to Radio Replacement.
4. Remove the instrument panel center speaker grille panel.
5. Remove the screws and the driver information bezel.
6. Remove the screws and the driver information center.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the driver information center with the screws and tighten to 2 N·m (18 lb in).
2. Install the driver information bezel with the screws and tighten to 2 N·m (18 lb in).
3. Install the instrument panel center speaker grille panel.
4. Install the radio. Refer to Radio Replacement.
5. Install the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement.
6. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.