For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the electrical connectors.
3. Remove the tail lamp assembly. Refer to Tail Lamp Replacement.
4. Remove any inoperative bulb.

### Installation Procedure

1. Install the replacement bulbs.
2. Install the tail lamp assembly. Refer to Tail Lamp Replacement.
3. Connect the electrical connectors.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.