For 1990-2009 cars

### Removal Procedure

1. Remove the outside rearview mirror cover.
2. Remove the bolts and the outside rearview mirror from the door.
3. Disconnect the mirror electrical connector, if equipped.

### Installation Procedure

1. Connect the mirror electrical connector, if equipped.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the outside rearview mirror bolts.

Tighten
Tighten the bolts to 10 N·m (85 lb in).

3. Install the outside rearview mirror cover.
4. Inspect the mirror for proper operation.