For 1990-2009 cars

1. Remove the second clutch sprag outer race thrust washer (506) from the second clutch sprag outer race assembly (505).
2. Remove the second coast clutch hub (500) from the second clutch sprag outer race assembly (505).
3. Remove the coast clutch hub thrust washer (501) from the second clutch sprag outer race assembly (505).
4. Remove the second clutch sprag end bearing (502).
5. Remove the second clutch sprag assembly (503).
6. Remove the second clutch end bearing (502).