For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor and Alternator Bracket Bolt | 35 N·m | 25.8 lb ft
A/C Compressor Lower Bolt | 23 N·m | 17 lb ft
Accessory Belt Idler Bolt | 52 N·m | 38.4 lb ft
Air Cleaner Assembly Bolt | 6 N·m | 53.1 lb in
Air Cleaner Upper Housing Screw | 2 N·m | 17.7 lb in
Beauty Cover Bolt | 8 N·m | 70.8 lb in
Beauty Cover Bracket Bolt | 11 N·m | 97.4 lb ft
Bed Plate Inner Bolt | 25+45°+90°N·m | 18.4+45°+90° lb ft
Bed Plate Outer Bolt | 35 N·m | 25.8 lb ft
Camshaft Cap Bolt | 28 N·m | 20.7 lb ft
Camshaft Sprocket Bolt | 133 N·m | 98.1 lb ft
Charge Air Cooler Bolt | 8.5 N·m | 75.2 lb in
Charge Air Cooler Inlet Pipe | 8 N·m | 70.8 lb in
Connecting Rod Cap Bolt | 25+90°N·m | 18.4+90° lb ft
Coolant Return Pipe Retaining Bolt | 9 N·m | 79.7 lb in
CPS Target Wheel Bolt | 12 N·m | 8.9 lb ft
Cradle Mounting Bolt | 155 N·m | 114.3 lb ft
Cradle Support Bracket Bolt | 50 N·m | 36.9 lb ft
Crankshaft Balancer Bolts | 55 N·m | 40.6 lb ft
Crankshaft Holder Hole Cap Bolt | 30 N·m | 22.1 lb ft
Crankshaft Pulley Bolt | 34 N·m | 25.1 lb ft
Crankshaft Sprocket Nut | 235 N·m | 173.3 lb ft
Cylinder Head Bolt | 65+120°+120°N·m | 47.9+120°+12+0° lb ft
Cylinder Head Cover Bolt | 12 N·m | 8.9 lb ft
EGR Retaining Nut (Engine Wiring Harness Bracket Nut) | 20 N·m | 14.8 lb ft
Engine Block Ground Bolt | 25 N·m | 18.4 lb ft
Engine Lift Bracket Retaining Nut | 28 N·m | 20.7 lb ft
Engine Lift Stud | 28 N·m | 20.7 lb ft
Engine Mount Bracket Bolt | 45 N·m | 33.1 lb ft
Engine Mount Bracket Retaining Bolt | 50 N·m | 36.9 lb ft
Engine Mount Frame Side Bracket Retaining Bolt | 100 N·m | 73.8 lb ft
Engine Mount Frame Side Bracket Retaining Nut | 90 N·m | 66.4 lb ft
Engine Wiring Splice Pack Tightening Bolt | 15 N·m | 11.1 lb ft
Exhaust Manifold Heat Shield Nut and Bolt | 20 N·m | 14.8 lb ft
Exhaust Manifold Nuts | 33 N·m | 24.3 lb ft
Exhaust Manifold Stud | 16 N·m | 11.8 lb ft
Flexible Plate Tightening Bolt | 105 N·m | 77.4 lb ft
Flywheel Tightening Bolt | 105 N·m | 77.4 lb ft
Fuel Pipe-to-Common Rail Retaining Bolt | 10 N·m | 88.5 lb in
Fuel Pipe-to-Injection Pump Retaining Bolt (to Cylinder Head Cover) | 25 N·m | 18.4 lb ft
Fuel Pipe-to-Injection Pump Retaining Bolt (to Intake Manifold) | 9 N·m | 79.7 lb in
Function Block Retaining Bolt | 11 N·m | 97.4 lb in
Glow Plug Fuse Box Retaining Bolt | 10 N·m | 88.5 lb in
Glow Plug Module Retaining Nut | 14 N·m | 10.3 lb ft
Injection Pump Sprocket Nut | 70 N·m | 51.6 lb ft
Intake Manifold Bolts and Nuts | 23 N·m | 17 lb ft
Intake Manifold Stud | 16 N·m | 11.8 lb ft
Oil Filter Cap | 25 N·m | 18.4 lb ft
Oil Filter Housing Adapter Plate | 40 N·m | 29.5 lb ft
Oil Filter Housing Fitting Bolt | 50 N·m | 36.9 lb ft
Oil Level Indicator Tube Bolt | 11 N·m | 97.4 lb in
Oil Nozzle Tube Retaining Bolt | 23 N·m | 17.7 lb ft
Oil Pan Flange-to-Transaxle Bolts | 50 N·m | 36.9 lb ft
Oil Pan Tightening Bolt | 11 N·m | 97.4 lb in
Oil Pump Tightening Bolt | 24 N·m | 17.7 lb ft
Oil Strainer Bolt | 11 N·m | 97.4 lb in
PCV Valve Adapter Bolt | 11 N·m | 97.4 lb in
PCV Valve Bolt | 11 N·m | 97.4 lb in
Power Steering Bracket Retaining Bolt | 25 N·m | 18.4 lb ft
Power Steering Pump Bolt | 25 N·m | 18 lb ft
Resonator Assembly Retaining Bolt | 6 N·m | 53.1 lb in
Tensioner Retaining Bolt | 48 N·m | 35.4 lb ft
Timing Belt Idler Retaining Bolt | 52 N·m | 38.4 lb ft
Timing Belt Lower Cover Bolt | 11 N·m | 97.4 lb in
Timing Belt Rear Cover Bolt | 11 N·m | 97.4 lb in
Timing Belt Tensioner Bolt | 25 N·m | 18.4 lb ft
Timing Belt Upper Cover Bolt | 11 N·m | 97.4 lb in
Transaxle Front Mount Retaining Bolt | 50 N·m | 36.9 lb ft
Transaxle Front Mount to Transaxle Through Bolt | 90 N·m | 66.4 lb ft
Transaxle Rear Mount Bracket Retaining Bolt | 90 N·m | 66.4 lb ft
Transaxle Rear Mount Retaining Bolt | 90 N·m | 66.4 lb ft
Transaxle Rear Mount to Bracket Through Bolt | 90 N·m | 66.4 lb ft
Transaxle Tightening Bolt (Bed Plate-to-Transaxle) | 75 N·m | 55.3 lb ft
Turbocharger Inlet Duct Bolt | 3 N·m | 26.6 lb in
Water Pump Inlet Pipe Retaining Bolt | 23 N·m | 17 lb ft