For 1990-2009 cars

### Removal Procedure

1. Loosen the clamp and disconnect the air cleaner outlet hose from the air cleaner housing.
2. Remove the air cleaner element cover screws.
3. Remove the air cleaner element.

### Installation Procedure

1. Install the air cleaner element cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Tighten the air cleaner element cover screws.

Tighten
Tighten the air cleaner element cover screws to 2 N·m (18 lb in).