For 1990-2009 cars

### Removal Procedure

Important: Left - Hand Drive Shown, Right - Hand Drive Similar.

1. Remove the hood prime latch release handle. Refer to Hood Primary Latch Release Cable Replacement .
2. Remove the screw and the instrument panel lower left trim.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the instrument panel lower left trim.

Tighten
Tighten the instrument panel steering column opening pillar screw to 2 N·m (18 lb in).

2. Install the hood prime latch release handle. Refer to Hood Primary Latch Release Cable Replacement .