For 1990-2009 cars

Connector 1: | Accelerator Pedal Position (APP) Sensor
Connector 2: | A/C Refrigerant Pressure Sensor
Connector 3: | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Exhaust (LU1)
Connector 4: | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Intake (LU1)
Connector 5: | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Exhaust (LU1)
Connector 6: | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Intake (LU1)
Connector 7: | Camshaft Position (CMP) Sensor - Bank 1 Exhaust (LU1)
Connector 8: | Camshaft Position (CMP) Sensor - Bank 1 Intake (LU1)
Connector 9: | Camshaft Position (CMP) Sensor - Bank 2 Exhaust (LU1)
Connector 10: | Camshaft Position (CMP) Sensor - Bank 2 Intake (LU1)
Connector 11: | Crankshaft Position (CKP) Sensor (LU1)
Connector 12: | Engine Coolant Temperature (ECT) Sensor
Connector 13: | Engine Oil Level Sensor (LU1)
Connector 14: | Engine Oil Pressure (EOP) Sensor (LU1)
Connector 15: | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve
Connector 16: | Fuel Injector 1 (LU1)
Connector 17: | Fuel Injector 2 (LU1)
Connector 18: | Fuel Injector 3 (LU1)
Connector 19: | Fuel Injector 4 (LU1)
Connector 20: | Fuel Injector 5 (LU1)
Connector 21: | Fuel Injector 6 (LU1)
Connector 22: | Fuel Level Sensor - Primary/Fuel Pump Motor
Connector 23: | Fuel Level Sensor - Secondary
Connector 24: | Fuel Tank Pressure Sensor
Connector 25: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LU1)
Connector 26: | Heated Oxygen Sensor Bank-1 Sensor 2
Connector 27: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LU1)
Connector 28: | Heated Oxygen Sensor Bank 2 Sensor 2
Connector 29: | Ignition Coil 1 (LU1)
Connector 30: | Ignition Coil 2 (LU1)
Connector 31: | Ignition Coil 3 (LU1)
Connector 32: | Ignition Coil 4 (LU1)
Connector 33: | Ignition Coil 5 (LU1)
Connector 34: | Ignition Coil 6 (LU1)
Connector 35: | Knock Sensor 1 (LU1)
Connector 36: | Knock Sensor 2 (LU1)
Connector 37: | Mass Air Flow (MAF) Sensor
Connector 38: | Throttle Actuator Control (TAC) Module

### Accelerator Pedal Position (APP) Sensor

#### Connector Part Information

- OEM: 15326830
- Service: 88953153
- Description: 6-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Accelerator Pedal Position (APP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU | 1272 | Low Reference
B | 0.35 L-BU | 1162 | APP Sensor 2 Signal
C | 0.35 TN | 1274 | 5-Volt Reference 1
D | 0.35 WH/BK | 1164 | 5-Volt Reference 2
E | 0.35 D-BU | 1161 | APP Sensor 1 Signal
F | 0.35 BN | 1271 | Low Reference

### A/C Refrigerant Pressure Sensor

#### Connector Part Information

- OEM: 15477863
- Service: 88988301
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### A/C Refrigerant Pressure Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 Gy | -- | 5-Volt Reference 1
2 | 0.5 BN | -- | Low Reference
3 | 0.5 OG/BK | -- | A/C Refrigerant Pressure Sensor Signal

### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Exhaust (LU1)

#### Connector Part Information

- OEM: 15411401
- Service: 88988588
- Description: 2-Way F 090 II, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4025/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Exhaust (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 WH | -- | Powertrain Main Relay Fused Supply
2 | 0.8 L-GN/GN | -- | Camshaft Phaser Exhaust Solenoid 1-Control

### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Intake (LU1)

#### Connector Part Information

- OEM: 15411401
- Service: 88988588
- Description: 2-Way F 090 II, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4025/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Intake (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 WH | -- | Powertrain Main Relay Fused Supply
2 | 0.8 PU | -- | Camshaft Phaser Intake Solenoid 1-Control

### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Exhaust (LU1)

#### Connector Part Information

- OEM: 15411401
- Service: 88988588
- Description: 2-Way F 090 II, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4025/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Exhaust (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 WH | -- | Powertrain Main Relay Fused Supply
2 | 0.8 WH/BK | -- | Camshaft Phaser Exhaust Solenoid 2-Control

### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Intake (LU1)

#### Connector Part Information

- OEM: 15411401
- Service: 88988588
- Description: 2-Way F 090 II, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4025/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Intake (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 WH | -- | Powertrain Main Relay Fused Supply
2 | 0.8 OG/BK | -- | Camshaft Phaser Intake Solenoid 2-Control

### Camshaft Position (CMP) Sensor - Bank 1 Exhaust (LU1)

#### Connector Part Information

- OEM: 15339753
- Service: 88988595
- Description: 3-Way F Compact 2.8 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Camshaft Position (CMP) Sensor - Bank 1 Exhaust (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/RD | -- | Low Reference
2 | 0.5 GN | -- | Camshaft Position (CMP) Sensor Signal - Bank 1 Exhaust
3 | 0.5 GY | -- | 5-Volt Reference 1

### Camshaft Position (CMP) Sensor - Bank 1 Intake (LU1)

#### Connector Part Information

- OEM: 15339753
- Service: 88988595
- Description: 3-Way F Compact 2.8 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Camshaft Position (CMP) Sensor - Bank 1 Intake (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/RD | -- | Low Reference
2 | 0.5 OG | -- | Camshaft Position (CMP) Sensor Signal - Bank 2 Intake
3 | 0.5 GY | -- | 5-Volt Reference 1

### Camshaft Position (CMP) Sensor - Bank 2 Exhaust (LU1)

#### Connector Part Information

- OEM: 15339753
- Service: 88988595
- Description: 3-Way F Compact 2.8 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Camshaft Position (CMP) Sensor - Bank 2 Exhaust (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/RD | -- | Low Reference
2 | 0.5 PU | -- | Camshaft Position (CMP) Sensor Signal - Bank 2 Exhaust
3 | 0.5 GY | -- | 5-Volt Reference 1

### Camshaft Position (CMP) Sensor - Bank 2 Intake (LU1)

#### Connector Part Information

- OEM: 15339753
- Service: 88988595
- Description: 3-Way F Compact 2.8 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Camshaft Position (CMP) Sensor - Bank 2 Intake (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/RD | -- | Low Reference
2 | 0.5 YE | -- | Camshaft Position (CMP) Sensor Signal - Bank 2 Intake
3 | 0.5 GY | -- | 5-Volt Reference 1

### Crankshaft Position (CKP) Sensor (LU1)

#### Connector Part Information

- OEM: 13525738
- Service: 88988337
- Description: 3-Way F USCAR 064 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 33467-0005/23
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Crankshaft Position (CKP) Sensor (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY/WH | -- | Low Reference
2 | 0.5 WH | -- | Crankshaft Position Sensor Signal
3 | 0.5 BK | -- | 5-Volt Reference 2

### Engine Coolant Temperature (ECT) Sensor

#### Connector Part Information

- OEM: 15339756
- Service: 88988963
- Description: 2-Way F 2.8, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498054/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Engine Coolant Temperature (ECT) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/RD | -- | ECT Sensor Signal
2 | 0.5 YE | -- | Low Reference

### Engine Oil Level Sensor (LU1)

#### Connector Part Information

- OEM: 12065287
- Service: 88988301
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12103881/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12180559-1/J-35616-14 (GN)

#### Engine Oil Level Sensor (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/RD | -- | Low Reference
2 | 0.5 GN/WH | -- | 5-Volt Reference
3 | 0.5 BN | -- | Oil Level Sensor Signal

### Engine Oil Pressure (EOP) Sensor (LU1)

#### Connector Part Information

- OEM: 12065287
- Service: 88988301
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12103881/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12180559-1/J-35616-14 (GN)

#### Engine Oil Pressure (EOP) Sensor (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/RD | -- | Low Reference
2 | 0.5 GY | -- | 5-Volt Reference
3 | 0.5 BN/BK | -- | Oil Pressure Sensor Signal

### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve

#### Connector Part Information

- OEM: PKI 832229
- Service: N/A
- Description: 2-Way F Sealed

#### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH | -- | EVAP Canister Vent Solenoid Control
2 | PK | -- | Run/Crank Ignition 1 Voltage

### Fuel Injector 1 (LU1)

#### Connector Part Information

- OEM: 15305086
- Service: 15306318
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 1 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5291 | Ignition 1 Voltage
B | 0.5 TN | 1744 | Fuel Injector 1 Control

### Fuel Injector 2 (LU1)

#### Connector Part Information

- OEM: 15305086
- Service: 15306318
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 2 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5292 | Ignition 1 Voltage
B | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control

### Fuel Injector 3 (LU1)

#### Connector Part Information

- OEM: 15305086
- Service: 15306318
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 3 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5291 | Ignition 1 Voltage
B | 0.5 PK/BK | 1746 | Fuel Injector 3 Control

### Fuel Injector 4 (LU1)

#### Connector Part Information

- OEM: 15305086
- Service: 15306318
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 4 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5292 | Ignition 1 Voltage
B | 0.5 L-BU/BK | 844 | Fuel Injector 4 Control

### Fuel Injector 5 (LU1)

#### Connector Part Information

- OEM: 15305086
- Service: 15306318
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 5 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5291 | Ignition 1 Voltage
B | 0.5 TN/WH | 845 | Fuel Injector 5 Control

### Fuel Injector 6 (LU1)

#### Connector Part Information

- OEM: 15419715
- Service: 15306318
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 6 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5292 | Ignition 1 Voltage
B | 0.5 YE/BK | 846 | Fuel Injector 6 Control

### Fuel Level Sensor - Primary/Fuel Pump Motor

#### Connector Part Information

- OEM: KET MG641521
- Service: N/A
- Description: 5-Way F 090II Sealed

#### Fuel Level Sensor - Primary/Fuel Pump Motor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 PK | 239 | Run/Crank Ignition Voltage
2 | 0.5 BN/WH | 628 | Fuel Level Sensor Low
3 | 0.5 D-BU | 1936 | Primary Fuel Level Sensor
4 | 2 GY | 120 | Fuel Pump Supply Voltage
5 | 2 BK | 450 | Ground

### Fuel Level Sensor - Secondary

#### Connector Part Information

- OEM: 13527865
- Service: See Catalog
- Description: 4-Way F GT 280 Series, Sealed (NA)

#### Terminal Part Information

- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Fuel Level Sensor - Secondary

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.5 BN/WH | 6281 | Low Reference
4 | 0.5 L-BU | 1937 | Secondary Fuel Level Sensor Signal

### Fuel Tank Pressure Sensor

#### Connector Part Information

- OEM: PKI 832311
- Service: N/A
- Description: 3-Way F 150 Sealed

#### Fuel Tank Pressure Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN/WH | 6281 | Fuel Level Sensor Low
2 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
3 | 0.5 GY | 2709 | Fuel Tank Pressure Sensor 5-Volt Reference

### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LU1)

#### Connector Part Information

- OEM: 1928404900
- Service: 12176897
- Description: 6-Way F Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BU/GN | -- | Low Reference
2 | 0.8 WH | -- | Powertrain Main Relay Fused Supply
3 | 0.8 PU | -- | HO2S Bank 1 Sensor 1 - High Signal
4 | 0.8 OG | -- | HO2S Pump Current Bank 1 Sensor 1
5 | 0.5 PU/WH | -- | HO2S Heater Low Control Bank 1 Sensor 1
6 | 0.5 PU/WH | -- | HO2S Input Pump Current Bank 1 Sensor 1

### Heated Oxygen Sensor Bank-1 Sensor 2

#### Connector Part Information

- OEM: BOSCH 1928403453
- Service: N/A
- Description: 4-Way F Sealed

#### Heated Oxygen Sensor Bank-1 Sensor 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 5293 | Engine Main Relay Fused Control (4)
2 | 0.5 GY/WH | 3122 | Heated O2 Sensor Bank 2 (2)
3 | 0.5 BN/WH | 1669 | Heated O2 Low Signal Bank 2 (2)
4 | 0.5 PU/WH | 1668 | Heated O2 High Signal Bank 2 (2)

### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LU1)

#### Connector Part Information

- OEM: 1928404900
- Service: 12176897
- Description: 6-Way F Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/WH | -- | Low Reference
2 | 0.8 WH | -- | Powertrain Main Relay Fused Supply
3 | 0.8 PU/WH | -- | HO2S Bank 2Sensor 1 - High Signal
4 | 0.8 L-GN/GN | -- | HO2S Pump Current Bank 2 Sensor 1
5 | 0.5 BU | -- | HO2S Heater Low Control Bank 2 Sensor 1
6 | 0.5 WH | -- | HO2S Input Pump Current Bank 2 Sensor 1

### Heated Oxygen Sensor Bank 2 Sensor 2

#### Connector Part Information

- OEM: BOSCH 1928403453
- Service: N/A
- Description: 4-Way F Sealed

#### Heated Oxygen Sensor Bank 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 5293 | Engine Main Relay Fused Control (4)
2 | 0.5 OG/WH | 3223 | Heated O2 Sensor Bank 2 (2)
3 | 0.5 BN | 1671 | Heated O2 Low Signal Bank 2 (2)
4 | 0.5 PU | 1670 | Heated O2 High Signal Bank 2 (2)

### Ignition Coil 1 (LU1)

#### Connector Part Information

- OEM: 15466325
- Service: See Catalog
- Description: 4-Way F USCAR 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil 1 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | -- | Ignition 1 Voltage
2 | 0.5 PU | -- | IC 1 Control
3 | 0.5 PU | -- | Low Reference
4 | 0.5 BK | -- | Ground

### Ignition Coil 2 (LU1)

#### Connector Part Information

- OEM: 15466325
- Service: See Catalog
- Description: 4-Way F USCAR 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil 2 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | -- | Ignition 1 Voltage
2 | 0.5 OG/WH | -- | IC 2 Control
3 | 0.5 PK | -- | Low Reference
4 | 0.5 BK | -- | Ground

### Ignition Coil 3 (LU1)

#### Connector Part Information

- OEM: 15466325
- Service: See Catalog
- Description: 4-Way F USCAR 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil 3 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | -- | Ignition 1 Voltage
2 | 0.5 L-BU | -- | IC 3 Control
3 | 0.5 PU | -- | Low Reference
4 | 0.5 BK | -- | Ground

### Ignition Coil 4 (LU1)

#### Connector Part Information

- OEM: 15466325
- Service: See Catalog
- Description: 4-Way F USCAR 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil 4 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | -- | Ignition 1 Voltage
2 | 0.5 GN/WH | -- | IC 4 Control
3 | 0.5 PK | -- | Low Reference
4 | 0.5 BK | -- | Ground

### Ignition Coil 5 (LU1)

#### Connector Part Information

- OEM: 15466325
- Service: See Catalog
- Description: 4-Way F USCAR 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil 5 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | -- | Ignition 1 Voltage
2 | 0.5 GN | -- | IC 5 Control
3 | 0.5 PU | -- | Low Reference
4 | 0.5 BK | -- | Ground

### Ignition Coil 6 (LU1)

#### Connector Part Information

- OEM: 15466325
- Service: See Catalog
- Description: 4-Way F USCAR 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil 6 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | -- | Ignition 1 Voltage
2 | 0.5 BU/WH | -- | IC 6 Control
3 | 0.5 PK | -- | Low Reference
4 | 0.5 BK | -- | Ground

### Knock Sensor 1 (LU1)

#### Connector Part Information

- OEM: 15339756
- Service: 88988963
- Description: 2-Way F 2.8, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498054/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Knock Sensor 1 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | -- | Knock Sensor 2 Signal
2 | 0.5 BU | -- | Low Reference

### Knock Sensor 2 (LU1)

#### Connector Part Information

- OEM: 15339756
- Service: 88988963
- Description: 2-Way F 2.8, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498054/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Knock Sensor 2 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | -- | Knock Sensor 2 Signal
2 | 0.5 L-BU | -- | Low Reference

### Mass Air Flow (MAF) Sensor

#### Connector Part Information

- OEM: PED 15355207
- Service: N/A
- Description: 5-Way F GT 150 Sealed

#### Mass Air Flow (MAF) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Intake Air Temp Sensor Low Reference
2 | BN | -- | Intake Air Temp Sensor Signal
3 | BK/WH | -- | Signal Ground
4 | PK | -- | Run/Crank Ignition 1 Voltage
5 | YE | -- | Mass Air Flow Sensor Signal

### Throttle Actuator Control (TAC) Module

#### Connector Part Information

- OEM: 15355297
- Service: 19115594
- Description: 6-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Pins: A-F
- Terminal/Tray: 15326427/5
- Core/Insulation Crimp: Pins A-B - See Terminal Repair Kit
- Core/Insulation Crimp: Pins C-F - E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Throttle Actuator Control (TAC) Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.75 YE | -- | TAC Motor Control - 2
2 | 0.75 BN | -- | TAC Motor Control - 1
3 | 0.5 BN/YE | -- | Low Reference
4 | 0.5 D-GN | -- | TP Sensor 1 Signal
5 | 0.5 GY | -- | 5-Volt Reference
6 | 0.5 PU | -- | TP Sensor 2 Signal