For 1990-2009 cars

#### Special Tools

• | J-3289-20 Holding Fixture

• | J-45159 Holding Fixture

1. Install the body of the J 45159 with the two long bolts (1) to the transaxle.
2. Loosely install the arm and bolt (2) to the J 45159 body.

Caution: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the arm with the provided shorter bolt (3) to the transaxle. Tighten the J-45159 fixture to 25 N·m (18 lb ft) starting with bolt (3).
4. Install the J-45159 fixture in the J-3289-20 fixture .