For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the steering column cover. Refer to Steering Column Trim Cover Replacement.
3. Set the ignition key to ON position.
4. Disconnect the electrical connector.
5. Remove the ignition switch retaining screws.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the ignition switch retaining screws and tighten to 2.5 N·m (22 lb in).
2. Connect the electrical connector.
3. Install the steering column cover. Refer to Steering Column Trim Cover Replacement.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.