For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the windshield wiper transmission frame assembly. Refer to Windshield Wiper Transmission Replacement.

1 | Windshield Wiper Motor Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (71 lb in)
2 | Windshield Wiper Motor

#### Procedure

1. Using a J 39232 Wiper Linkage Separator or similar tool remove the transmission drive links from the wiper motor crank arm ball stud.
2. Using a J 39529 Wiper Linkage Installer or similar tool install the wiper transmission drive links onto the wiper motor crank arm ball stud.

Tip
Apply a small amount of grease to the inner cup on the transmission links to aid in installation.