For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the drain plug (1).
3. Remove the fill plug (2)

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the drain plug (1).

Tighten
Tighten the drain plug (1) to 39 N·m (29 lb ft).

2. Fill the transfer case with synthetic hypoid 75W-90 to the bottom of the fill plug hole, when the vehicle is on a level surface.
3. Install the fill plug (2).

Tighten
Tighten the fill plug (2) to 39 N·m (29 lb ft).

4. Lower the vehicle.