For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Engine Protection Shield Nut | 10 N·m | 89 lb in
Engine Shield Bolts | 2 N·m | 18 lb in
Fender Liner Screws | 4 N·m | 35 lb in
Front Suspension Crossmember Support Bracket to Body Bolts | 10 N·m | 89 lb in
Front Suspension Crossmember to Body Bolts | 155 N·m | 114 lb ft
Front Suspension Crossmember to Transmission Front Mount Bolts | 50 N·m | 37 lb ft
Front Suspension Crossmember to Transmission Rear Mount Bolt | 110 N·m | 81 lb ft
Mud Guard Bolts | 110 N·m | 81 lb ft
Outer Tie Rod to Knuckle Nut | 170 N·m | 125 lb ft
Power Steering Gear to Front Suspension Crossmember Bolts | 50 N·m | 37 lb ft
Rear Support to Body Bolts | 110 N·m | 81 lb ft
Stabilizer Link Nuts | 65 N·m | 48 lb ft
Stabilizer Shaft Clamp to Front Suspension Crossmember Bolts | 50 N·m | 37 lb ft
Transmission Front Mount to Transmission Bolt | 50 N·m | 37 lb ft
Wheel Nuts | 125 N·m | 92 lb ft