For 1990-2009 cars

## Scan Tool Data List Except Holden

The Engine Control Module Scan Tool Data List contains all ECM related parameters that are available on the scan tool. The list is arranged in alphabetical order. A given parameter may appear in any one of the data lists, and in some cases may appear more than once, or in more than one data list in order to group certain related parameters together.

Use the Engine Control Module Scan Tool Data List only after the following is determined:

• | The Diagnostic System Check - Vehicle is completed.

• | No diagnostic trouble codes (DTCs) are present.

• | The on-board diagnostics are functioning properly.

Scan tool values from a properly running engine may be used for comparison with the engine you are diagnosing. The Engine Control Module Scan Tool Data List represents values that would be seen on a normal running engine.

Important: A scan tool that displays faulty data should not be used. The scan tool problem should be reported to the manufacturer. Use of a faulty scan tool can result in misdiagnosis and unnecessary parts replacement.

The column labeled Data List indicates where a parameter can be located on the scan tool. Refer to the scan tool operating manual for the exact locations of the data lists. The following is a description of each term listed:

All: The parameter is in all of the data lists indicated below.
Eng: Engine Data List
CH: Cooling/HVAC Data List
CC: Cruise Control Data List
EGR: Exhaust Gas Recirculation (EGR) Data List
ET: Electrical/Theft Data List
EA: Exhaust Aftertreatment Data List
Fuel: Fuel Data List
Induction: Induction Data List

#### Scan Tool Data List

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Engine Idling/Lower Radiator Hose Hot/Closed Throttle/Park or Neutral/Accessories Off
5 Volt Reference 1, Reference 2, or Reference 3 Circuit Status | CH, EGR, EA, Fuel, Induction | OK/Fault | OK
A/C Disengage Reason | CH | Accel Rate/Acceleration/Coolant Temp/High Pressure/Invalid/Low Pressure/System Voltage | Invalid
A/C Refrigerant Pressure | CH | kPa/PSI | Varies
A/C Refrigerant Pressure | CH | Volts | Varies
A/C Relay Command | Eng, CH, EGR, Induction | ON/OFF | Off
A/C Request Signal | CH | Yes/No | No
A/C High Side Press. SW | CH | Normal/High Pressure | Normal
Alternator L Terminal | ET | ON/OFF | ON
Ambient Air Temperature Calculated | Eng | °C/°F | Varies
APP at Idle | Induction | No/Yes | Yes
APP Sensor 1 or Sensor 2 | Induction | Volts | Varies
APP Sensor 1 or Sensor 2 Indicated | Eng, CC, EGR, ET, EA, Fuel, Induction | % | Varies
APP Sensors | ET | % | Varies
Auto Learn Counter | ET | Counts | Varies
Aux Htr. Relay 1 Command | CH | ON/OFF | OFF
Aux Htr. Relay 2 and 3 Command | CH | ON/OFF | OFF
Aux Heater Request | CH | ON/OFF | OFF
BARO | Eng, EGR, EA, Fuel, Induction | kPa | Varies
BARO | Induction | Volts | Varies
Battery Voltage | All | Volts | Varies
Boost Pressure Sensor | Eng, Induction | kPa/PSI | Varies
Boost Pressure Sensor | Induction | Volts | Varies
Calculated Mass Air Flow | Induction | Grams/second | Varies
Clutch Pedal Switch (If Equipped) | CC, ET | Released/Applied | Applied
Cruise Control Active | Eng, CC | Yes/No | No
Cruise Disengage 1-6 History | CC | Reason | Varies
Cruise ON/OFF Switch | CC | ON/OFF | OFF
Cruise Release Brake Pedal Switch | Eng, CC, ET | Released/Applied | Released
Cruise Resume/Accel. Switch | CC | ON/OFF | OFF
Cruise Set/Coast Switch | CC | ON/OFF | OFF
Cylinder Air | Induction | mg/stk | Varies
Desired Boost | Induction | kPa | Varies
Desired Cylinder Air | Induction | mg/stk | Varies
Desired Fuel Rail Pressure | Fuel | kPa/PSI | Varies
Desired Idle Speed | Eng, CC, EA, Fuel, Induction | RPM | 700-800
Distance Since Last DPF Regeneration | EA | Miles/Km | Varies
Distance Since DPF Indicator ON without Regeneration | EA | Miles/Km | Varies
DPF Flow Calculated | EA | Liters/Hour | Varies
DPF Indicator Command | EA | ON/OFF | OFF
DPF Regen Command | EA | Counts | Varies
DPF Regen Flow Resistance | EA |  |
DPF Regeneration Inhibit | EA | Yes/No | No
DPF Regen Interrupted | EA | Yes/No | No
DPF Soot Mass | EA | Grams | Varies
ECM Authentication Status | ET | Valid/Invalid | Valid
ECM Challenge Status | ET | Valid/Invalid | Invalid
ECM Response Source | ET | Normal/Remote Start | Normal
ECT Sensor | All | °C/°F | Varies
ECT Sensor | ET | Volts | Varies
EGR Position Command | EGR, Induction | % | Varies
EGR Solenoid Command | Eng, EGR, Fuel | ON/OFF | OFF
EGT Sensor 1 or Sensor 2 | Eng, EA, Induction | °C/°F | Varies
EGT Sensor 1 or Sensor 2 | EA | Volts | Varies
Engine Load | Eng, CH, EGR, EA, Fuel, Induction | % | Varies
Engine Oil Level Switch | Eng, CC, ET, | OK/Low | OK
Engine Oil Pressure Switch | Eng, ET | OK/Low | OK
Engine Run Time | Eng , CH, CC, EGR, Fuel, Induction | Hrs/Mins/Sec | Varies with engine run time
Engine Speed | All | RPM | +/-50 RPM from desired
Fan Control 1, Control 2, or Control 3 Command | CH | ON/OFF | OFF
Fuel Heater Command | Fuel | ON/OFF | OFF
Fuel Level | Eng, EA, Fuel | % | Varies
Fuel Level Sensor Left Tank or Fuel Level Sensor Right Tank | Fuel | Volts | Varies
Fuel Pressure Regulator 1 | Eng, Fuel | mA | 1330
Fuel Pressure Regulator 2 | Eng, Fuel | mA | 525
Fuel Pressure Regulator 2 Command | Eng, Fuel | % | 20%
Fuel Pump Command | Eng, Fuel | % | 34%
Fuel Pump Relay | Eng, Fuel | ON/OFF | ON
Fuel Rail Pressure Sensor | Eng, Fuel | kPa/PSI | Varies
Fuel Rail Pressure Sensor | Fuel | Volts | Varies
Fuel Temperature Sensor | Eng, Fuel | °C/°F | Varies
Fuel Temperature Sensor | Fuel | Volts | Varies
GEN F Terminal Signal | ET | % | Varies
Glow Plug | Induction | % | Varies
Glow Plug Command | Eng, Induction | ON/OFF | OFF
Glow Plug Lamp Command | Induction | ON/OFF | OFF
IA Flow Valve Motor Command | EA, EGR, Induction | % | Varies
IAT Sensor 1 or Sensor 2 | Eng, CH, EGR, EA, Fuel, Induction | -39 to +140°C (-38 to +294°F) | Varies
Ignition 0 | Eng, ET | Active/Inactive | Active
Ignition 1 | Eng , CH, CC, ET, Fuel, Induction | Active/Inactive | Active
Immobilizer Programmed | ET | Yes/No | Yes
Immobilizer State | ET | Incorrect/No Comm/Negative/Post Release/Pre Release/Standby/Start Disable/Released | Released
MAF Sensor | Eng, EGR, EA, Fuel, Induction | g/s | 5-7
Main Injection Fuel Ratio | Eng, Fuel | mm³ | Varies
Main Injection Timing | Eng, Fuel | Degrees | 0 ± 3 degrees
MAP Sensor | Eng, EGR, EA, Fuel, Induction | kPa | Near BARO
MIL Command | Eng, EA, Fuel | ON/OFF | OFF
Particulate Filter Pressure Variance | EA | kPa/PSI | Varies
Particulate Filter Pressure Variance | EA | Volts | Varies
Pilot Injection Trim Average | Fuel | microseconds | Varies
Pilot Injection Trim Cyls 1-4 | Fuel | microseconds | Varies
PNP Switch (If Equipped) | Eng, ET | Park/ Net/ In Gear | Varies
Security Code Programmed | ET | Yes/No | Yes
Starter Relay Command | ET | ON/OFF | OFF
Stoplamp Pedal Switch | CC, ET | Applied/Released | Released
TC Vane Pos. Ctrl. Solenoid | Eng, Induction | % | Varies
Throttle Position | Eng, CC, EGR, EA, Fuel, Induction | % | Varies
Vehicle Speed | All | km/h/mph | 0 km/h (0 mph)
VTD Password Learn Enabled | ET | Yes/No | No
VTD security Code Accepted | ET | Yes/No | No
VTD security Code Lockout | ET | Active/Inactive | Active
Water In Fuel | Fuel | ON/OFF | OFF

## Scan Tool Data List Holden

The Engine Control Module Scan Tool Data List contains all ECM related parameters that are available on the scan tool. The list is arranged in alphabetical order. A given parameter may appear in any one of the data lists, and in some cases may appear more than once, or in more than one data list in order to group certain related parameters together.

Use the Engine Control Module Scan Tool Data List only after the following is determined:

• | The Diagnostic System Check - Vehicle is completed.

• | No diagnostic trouble codes (DTCs) are present.

• | The on-board diagnostics are functioning properly.

Scan tool values from an engine that is operating correctly may be used for comparison with the engine you are diagnosing. The Engine Scan Tool Data List represents the values that would be seen on a normal operating engine under the conditions specified in the first row of the Scan Tool Data List table.

Important: Do not use a scan tool that displays faulty data. The scan tool concern should be reported to the manufacturer. Use of a faulty scan tool may result in misdiagnosis and unnecessary parts replacement.

#### Scan Tool Data List

Scan Tool Parameter | System State | Expected Value | Description
--- | --- | --- | ---
Engine Idling / Operating Temperature / Closed Throttle / Park or Neutral / Closed Loop / Accessories Off
A/C Cutoff Mode (Air Conditioning) | System OK High Pressure Low Pressure A/C Pressure High Engine Temp

Low Engine Temp

Engine Temp

Max Torque

Max Acceleration

Not Programmed

-

This parameter displays the A/C cutoff mode status.

A/C Information Switch (Air Conditioning) | Inactive Active Not Programmed | - | This parameter displays the A/C Information switch status.
A/C Pressure (Air Conditioning) | - | kPa | This parameter displays the pressure in KPA from the A/C high side pressure sensor signal circuit to the control module.
A/C Pressure (Air Conditioning) | - | V | This parameter displays the voltage from the A/C high side pressure sensor signal circuit to the control module.
A/C Relay (Air Conditioning) | Inactive Active Not Programmed | - | This parameter displays the state of the air conditioning (A/C) clutch relay control circuit as commanded by the control module.
Ambient Temperature | - | °C | This parameter displays the calculated ambient air temperature.
APP at Idle Position (Accelerator Pedal Position) | Active Inactive | - | This parameter displays Active if an angle of the accelerator pedal at idle is calculated by the control module using the signals from the accelerator pedal position sensors.
APP Sensor 1 (Accelerator Pedal Position) | - | V | This parameter displays the voltage of the APP sensors signal circuits as measured by the control module.
APP Sensor 2 (Accelerator Pedal Position)
B1S1 Exhaust Gas Temperature (Bank 1 Sensor 1) | - | °C | This parameter displays the Degrees of the Exhaust Gas Temperature as measured by the control module.
B1S2 Exhaust Gas Temperature (Bank 1 Sensor 2)
B1S1 Exhaust Gas Temperature (Bank 1 Sensor 1) | - | V | This parameter displays the voltage of the Exhaust Gas Temperature as measured by the control module.
B1S2 Exhaust Gas Temperature (Bank 1 Sensor 2)
Barometric Pressure | - | kPa | This parameter displays the barometric pressure in KPA.
Barometric Pressure | - | V | This parameter displays the barometric pressure in Voltage.
Battery Voltage | - | V | This parameter displays 0 to 30 Volts. The voltage measured between the module’s battery positive voltage circuit and ground circuit.
Boost Pressure | - | kPa | This parameter indicates the turbocharger boost pressure inside the engine as calculated by the control module based on the signal from the Boost pressure sensor. The scan tool will display a higher value under heavy load, and a lower value at idle.
Boost Pressure | - | V | This parameter indicates the turbocharger boost pressure inside the engine in voltage as calculated by the control module based on the signal from the Boost pressure sensor. The scan tool will display a higher voltage under heavy load, and a lower voltage at idle.
Boost Pressure Command | - | kPa | This parameter displays the pressure of the Boost Pressure Command.
Brake Switch 1 | Inactive Active | - | This parameter displays the status of the Brake switch's as measured by the control module.
Brake Switch 2 | Inactive Active Not Programmed
Calculated Air Flow | - | kg/h | This parameter displays the calculated air flow into the engine. The calculation is used in several diagnostics to determine when to run the diagnostics.
Calculated Pedal Position | - | % | This parameter displays the percentage of the Calculated Pedal Position as measured by the control module.
Camshaft Speed | - | RPM | This parameter displays the RPM of the Camshaft based on input to the control module from the Camshaft sensor.
Charge Air Temperature | - | °C | This parameter displays the Degrees of the Charge Air Temperature as measured by the control module.
Charge Air Temperature | - | V | This parameter displays the voltage of the Charge Air Temperature as measured by the control module.
Common Rail Fuel Pressure | - | Mpa | This parameter displays the common fuel rail pressure in Mpa as calculated by the control module using the signal from the fuel rail pressure (FRP) sensor.
Common Rail Fuel Pressure | - | V | This parameter displays the common fuel rail pressure in voltage as calculated by the control module using the signal from the fuel rail pressure (FRP) sensor.
Coolant Temperature | - | °C | This parameter displays the temperature of the engine coolant based on input to the control module from the engine coolant temperature (ECT) sensor.
Coolant Temperature | - | V | This parameter displays the voltage of the engine coolant based on input to the control module from the engine coolant temperature (ECT) sensor.
Cruise Control | Inactive Active Not Programmed | - | This parameter displays the Status of the Cruise control.
Cruise Control Tip Switch | Inactive I (set) R (resume) Invalid (I+R) O (off)

I+O

R+O

Not Programmed

-

This parameter displays the status of the Cruise Control Tip Switch.

Desired Common Rail Fuel Pressure | - | Mpa | This parameter displays the desired common fuel rail pressure in Mpa.
Desired Engine Idle Speed | - | RPM | This parameter displays the desired engine idle speed.
Diagnosis Glow Time Relay | Active Inactive | - | This parameter displays the status of the diagnosis glow time relay.
Diesel Particulate Filter Saturation | - | % | This parameter displays the percentage calculated by the control module, based on the input from the exhaust gas temperature sensors.
Differential Pressure Diesel Particulate Filter | - | kPa | This parameter displays the kPa calculated by the control module, based on the input from the exhaust gas temperature sensors.
Differential Pressure Diesel Particulate Filter | - | V | This parameter displays the voltage calculated by the control module, based on the input from the exhaust gas temperature sensors.
Dist. Since Last DPF Regeneration (Distance) | - | km | This parameter displays the km since the last diesel particulate filter regeneration has occurred.
EGR Cooler Bypass Solenoid Valve Pulse Ratio (Exhaust Gas Recirculation) | - | % | This parameter displays the percentage of the EGR cooler bypass solenoid valve pulse ratio.
EGR Position Commanded (Exhaust Gas Recirculation) | - | % | This parameter displays the duty cycle commanded by the control module for the EGR valve.
EGR Pulse Ratio (Exhaust Gas Recirculation) | - | % | This parameter displays the percentage of the EGR pulse ratio.
Engine Oil Level Status | Okay Warning Warning Quit History Warning Disabled

Not Used

Not Programmed

-

This parameter displays the status of the engine oil level switch as determined by the control module.

Engine Speed | - | RPM | This parameter displays the speed of the engine crankshaft rotation from information received from the crankshaft position (CKP) sensor.
Engine Torque | - | Nm | This parameter displays the calculated engine load in Nm based on inputs to the control module from various engine sensors.
Fan Control 1 | Active Inactive | - | This parameter displays the control module commanded state of the cooling fans.
Fan Control 2 | Active Inactive | -
Final Fuel Injection Amount | mm3 stk | - | This parameter displays the final fuel injection amount.
Fuel Level Sensor 1 (Right) | - | V | This parameter displays the voltage signal received by the control module from the fuel level sensor Right.
Fuel Level Sensor 2 (Left) | - | V | This parameter displays the voltage signal received by the control module from the fuel level sensor Left.
Fuel Metering Solenoid Valve Current | - | A | This parameter displays the Fuel Metering Solenoid Valve Current.
Fuel Metering Solenoid Valve PWM | - | % | This parameter displays the Fuel Metering Solenoid Valve PWM.
Fuel Pump Relay | Active Inactive | - | This parameter displays the control modules commanded state of the fuel pump relay control circuit.
Fuel Temperature | - | °C | This parameter displays the Degrees of the fuel temperature as calculated by the control module based on input from the fuel temperature sensor.
Fuel Temperature | - | V | This parameter displays the voltage as calculated by the control module based on input from the fuel temperature sensor.
Glow Time Telltale | Off 12V On 0V | - | This parameter displays the commanded state of the glow plug lamp circuit by the control module.
Heater Relay 1 (Additional Electrical) | Active Inactive | - | This parameter displays the status of the heater relays .
Heater Relay 2 (Additional Electrical) | Active Inactive
Idle Speed Modified | Yes No | - | This parameter displays the idle speed modified status.
Ignition Status | On 12V Off 0V | - | This parameter displays the ignition status.
Intake Air Temperature | - | °C | This parameter displays the temperature of the air entering the air induction system based on input to the control module from the intake air temperature (IAT) sensor.
Main Injection Timing | - | °CA | This parameter displays the amount of main injection timing.
Malfunction Indicator (MI) | Off On Flashing | - | This parameter displays the commanded state of the malfunction indicator lamp (MIL) control circuit.
Mass Air Flow Sensor | - | kg/h | This parameter displays the measured quantity of air flowing into the engine during all operating conditions.
Odometer Value | - | km | This parameter displays the distance the vehicle has traveled in Km.
Oil Level | Normal Low Not Programmed | - | This parameter displays the status of the engine oil level switch as determined by the control module.
Oil Pressure | Normal Low Pressure | - | This parameter displays the pressure of the engine oil as calculated by the control module using a signal from the engine oil pressure (EOP) sensor.
Pulse Ratio Boost Pressure Solenoid Valve | - | % | This parameter displays the percentage of the pulse ratio boost pressure solenoid valve.
Rail Pressure Control Solenoid Valve Current | - | A | This parameter displays the Amps of the rail pressure control solenoid valve current.
Rail Pressure Control Solenoid Valve PWM | - | % | This parameter displays the percentage of the rail pressure control solenoid valve PWM.
Requested Torque (Traction Control) | - | Nm | This parameter displays the requested torque in Nm.
Service Vehicle Soon (SVS) Indicator | Off On Flashing | - | This parameter displays the status of the service vehicle soon indicator.
Starter Relay | Active Inactive | - | This parameter displays the commanded state of the starter relay. The scan tool will display Active or Inactive.
Throttle Position PWM Servo Signal | - | % | This parameter displays the percent of throttle opening as calculated by the control module using information from the TP sensor.
Torque Control | Active Inactive | - | This parameter displays the status of the torque control.
Vehicle Acceleration | - | m/s2 |
Vehicle Speed | - | km/h | This parameter displays the speed of the vehicle as calculated by the control module from information received from the vehicle speed sensor (VSS).
Vehicle Speed in Cruise Control Range | Inactive Active Not Programmed | - | This parameter displays the status of the vehicle speed in cruise control range.