For 1990-2009 cars

### Removal Procedure

1. Remove the seatback. Refer to Front Seat Back Replacement.
2. Remove the seat trim. Refer to Front Seat Trim Panel Replacement.
3. Remove the seat cushion bolts.
4. Remove the seat track from the seat cushion.

### Installation Procedure

1. Install the cushion onto the seat track.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the seat track to the seat cushion with the seat cushion bolts.

Tighten
Tighten the front seat cushion bolts to 12 N·m (9 lb ft).

3. Install the seat trim. Refer to Front Seat Trim Panel Replacement.
4. Install the seatback. Refer to Front Seat Back Replacement.