For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the air inlet grille panels. Refer to Air Inlet Grille Panel Replacement

1 | Windshield Wiper Transmission Frame Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (71 lb in)
2 | Windshield Wiper Transmission Frame Assembly

#### Procedure

1. Disconnect the windshield wiper motor electrical connector.
2. Roll the frame assembly forward in order to release the transmission frame assembly from the upper plenum supports.
3. Remove the windshield wiper motor from the wiper transmission frame assembly. Refer to Windshield Wiper Motor Replacement.