For 1990-2009 cars

Checks | Causes
--- | ---
2-6 Clutch Assembly |

• | Inspect for damaged or worn 2-6 Clutch Plates (540-542)

• | Inspect for damaged, worn, broken, improper surface finish or sheared splines on the Low-Reverse Clutch Assembly (543)

• | Inspect for damaged or broken 2-6 Clutch Piston (535) and piston seals damaged, worn or delaminating

• | Inspect for broken or binding 2-6 clutch Piston Return Spring (536)

Reaction Carrier Assembly (567) |

• | Inspect for stripped or sheared splines on the Input Ring Gear

• | Inspect for disengaged or broken Input Ring Gear Retainer

Reaction Sun Gear Assembly (566) |

• | Inspect for damaged or broken Reaction Sun Gear Assembly hub

• | Inspect for damaged or broken sun gear weld

• | Inspect for loose or worn Reaction Sun Gear Assembly bushing

Case Assembly (50) |

• | Inspect for stripped or sheared splines

• | Inspect for broken or disengaged 2-6 Clutch Piston Return Spring Retainer (537)

• | Inspect for damaged, worn, or improper surface finish in the piston bore