For 1990-2009 cars

Checks | Causes
--- | ---
Torque Converter (28) | Inspect for damage
Case Assembly (50) |

• | Inspect for cracked or broken Case (50)

• | Inspect for porosity or damage on the sealing surfaces

• | Inspect for loose Oil Cooler Line Bolts or damaged Oil Cooler Line Seals

• | Inspect for damaged Manual Shift Shaft Seal (604)

• | Inspect for damaged or worn Axle Seal (65) or Axle Seal Slinger on the axle shafts

• | Inspect for plugged Vent Cap (52)

• | Inspect for loose Pressure Test Plug (51), Drain Plug (64) and Fluid Level Plug (63)

• | Inspect for damaged Park Pawl Actuator Guide Seal (605)

• | Inspect for damaged or worn Input Speed Sensor Seals (19)

Torque Converter Housing Assembly (208) |

• | Inspect for damaged Torque Converter Housing Assembly (208)

• | Inspect for porosity or damage on the sealing surfaces

• | Inspect for damaged Torque Converter Housing Seal (23)

• | Inspect for damaged or worn Torque Converter Fluid Seal (301)

• | Inspect for loose Torque Converter and Differential Housing Bolts (26)

• | Inspect for damaged or worn Axle Seal (209) or Axle Seal Slingers on the axle shafts

• | Inspect for loose, missing or damaged Fluid Fill Tube Plug Assembly (27)

• | Inspect for damaged Torque Converter and Differential Housing Seal (202)

Valve Body Cover Assembly (2) |

• | Inpsect for damaged or warped Valve Body Cover Assembly (2)

• | Inspect for damaged or improperly installed Valve Body Cover Gasket (3)

• | Inspect for loose Valve Body Cover Bolts (1)

• | Inspect for damaged or improperly installed Wire Connector Hole Seal (5)