For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the electrical connectors.
3. Remove the nuts and the lamp assembly.
4. Remove any inoperative bulb.

### Installation Procedure

1. Install the replacement bulbs.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the lamp assembly with the nuts and tighten to 2.5 N·m (22 lb in).
3. Connect the electrical connectors.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.