For 1990-2009 cars

## Grille Replacement C100/Long Body

### Removal Procedure

1. Open the hood.
2. Remove the nuts and the radiator grille.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the radiator grille with the nuts.

Tighten
Tighten the radiator grille nuts to 4.5 N·m (40 lb in).

2. Close the hood.

## Grille Replacement C105/Short Body

### Removal Procedure

1. Open the hood.
2. Remove the nuts and the radiator grille.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the radiator grille with the nuts.

Tighten
Tighten the radiator grille nuts to 4.5 N·m (40 lb in).

2. Close the hood.