For 1990-2009 cars

## Rear Bumper Fascia Replacement C 100/Long Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the connector of the rear object sensor, if equipped.
3. Remove the bolts on the rear wheelhouse liner.
4. Remove the rear lower fascia retainers.
5. Remove the fascia.
6. Remove the tail lamps. Refer to Tail Lamp Replacement.
7. Remove the upper fascia screws and retainers.
8. Remove the rear bumper fascia from the rear quarter panel by pulling the side of the fascia outward.
9. Remove the rear bumper fascia from the vehicle.

### Installation Procedure

1. Install the rear bumper fascia to the vehicle.
2. Install the side of the rear bumper fascia to the rear quarter panel.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the upper fascia screws and retainers.

Tighten
Tighten the rear upper fascia screws to 2 N·m (18 lb in).

4. Install the tail lamps. Refer to Tail Lamp Replacement
5. Install the lower fascia retainers.
6. Install the bolts on the rear wheelhouse liner.

Tighten
Tighten the rear wheelhouse liner bolts to 4 N·m (36 lb in).

7. Connect the connector of the rear object sensor, if equipped.
8. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

## Rear Bumper Fascia Replacement C 105/Short Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the connector of the rear object sensor, if equipped.
3. Remove the bolts on the rear wheelhouse liner.
4. Remove the rear lower fascia retainers.
5. Remove the fascia.
6. Remove the tail lamps. Refer to Tail Lamp Replacement.
7. Remove the upper fascia screws and retainers.
8. Remove the rear bumper fascia from the rear quarter panel by pulling the side of the fascia outward.
9. Remove the rear bumper fascia from the vehicle.

### Installation Procedure

1. Install the rear bumper fascia to the vehicle.
2. Install the side of the rear bumper fascia to the rear quarter panel.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the upper fascia screws and retainers.

Tighten
Tighten the rear upper fascia screws to 2 N·m (18 lb in).

4. Install the tail lamps. Refer to Tail Lamp Replacement
5. Install the lower fascia retainers.
6. Install the bolts on the rear wheelhouse liner.

Tighten
Tighten the rear wheelhouse liner bolts to 4 N·m (36 lb in).

7. Connect the connector of the rear object sensor, if equipped.
8. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.