For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

Important: Only lift the engine far enough to take the weight off the transaxle rear mount assembly, or damage to the mount and lifting equipment failure may occur.

1. Support the engine assembly using DW-110-060 .
2. Remove the transaxle rear mount-to-bracket through bolt.
3. Remove the transaxle rear mount bracket retaining bolts from the transaxle.
4. Remove the transaxle rear mount bracket.
5. Remove the transaxle rear mount retaining bolts from the cradle.
6. Remove the transaxle rear mount.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the transaxle rear mount to the cradle.

Tighten
Tighten the transaxle rear mount retaining bolts to 90 N·m (66 lb ft).

2. Install the transaxle rear mount bracket to the transaxle.

Tighten
Tighten the transaxle rear mount bracket retaining bolts to 90 N·m (66 lb ft).

Important: Before tightening the transaxle rear mount through bolt, swing the engine assembly backwards and forwards or from the side to side for the proper alignment.

3. Install the transaxle rear mount through bolt.

Tighten
Tighten the transaxle rear mount to bracket through bolt to 90 N·m (66 lb ft).

4. Remove the engine support fixture DW-110-060 .