For 1990-2009 cars

1. Loosen the upper control arm-to-frame fastener enough to allow movement.

Important: The frame of the vehicle is slotted, turning the cam nut will move the camber in to the designated location.

2. Rotate the upper control arm-to-frame fastener in the direction necessary to the correct the camber measurement.
3. Snug the upper control arm-to-frame fastener, do not tighten at this time.
4. Reinspect the rear camber specifications and adjust as necessary.

Notice: Refer to Fastener Notice in the Preface section.

5. Hold the nut and tighten the upper control arm-to-frame bolt.

Tighten
Tighten the bolt to 164 N·m (121 lb ft).

6. Repeat the procedure for the other rear wheel.