For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front floor console. Refer to Console Replacement.
2. Disconnect the range select cable from range select lever.
3. Disconnect the range select lever electrical connector.

1 | Automatic Transmission Range Select Lever Nut (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (71 lb in)
2 | Automatic Transmission Range Select Lever