For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Loosen the stabilizer shaft clamp bolts.

Note: When disconnecting the stabilizer link, hold the link with a wrench to prevent turning.

3. Remove the stabilizer link to stabilizer shaft nut.

Note: When disconnecting the stabilizer link, hold the link with a wrench to prevent turning.

4. Remove the stabilizer link to lower control arm nut.
5. Remove the stabilizer link from the vehicle.

### Installation Procedure

1. Position the stabilizer link through the lower control arm.

Caution: Refer to Fastener Caution in the Preface section.

Note: When connecting the stabilizer link, hold the link with a wrench to prevent turning.

2. Install the stabilizer link to control arm nut and tighten to 15 N·m (11 lb ft).
3. Install the stabilizer link to stabilizer shaft nut and tighten to 57 N·m (42 lb ft).
4. Tighten the stabilizer shaft clamp bolts and tighten to 70 N·m (52 lb ft).
5. Lower the vehicle.