For 1990-2009 cars

## Sunshade Replacement C100/Long Body

### Removal Procedure

1. Remove the screws and the sunshade from the headliner.
2. Disconnect the vanity mirror electrical connector.
3. Remove the screw and the sunshade support from the headliner.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the sunshade support to the headliner with the screw and tighten to 3 N·m (27 lb in).
2. Connect the vanity mirror electrical connector.
3. Install the sunshade to the headliner with the screws and tighten to 3 N·m (27 lb in).

## Sunshade Replacement C105/Short Body

### Removal Procedure

1. Remove the sunshade bracket cover.
2. Remove the screws and the sunshade from the headliner.
3. Disconnect the vanity mirror electrical connector.
4. Remove the screw and the sunshade support from the headliner.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the sunshade support to the headliner with the screw and tighten to 3 N·m (27 lb in).
2. Connect the vanity mirror electrical connector.
3. Install the sunshade bracket to the headliner with the screws and tighten to 3 N·m (27 lb in).
4. Install the sunshade bracket cover.