For 1990-2009 cars

Bleed the hydraulic system to remove air which entered when the pipes were disconnected for repairs. The clutch fluid in the clutch reservoir must be maintained at the MIN level or higher during air bleeding.

1. Attach a vinyl hose to the bleeder plug. Place the other end of the vinyl tube in a glass container half filled with clutch fluid.
2. Slowly pump the clutch pedal several times
3. While you press the clutch pedal, loosen the bleeder screw until the fluid starts to run out. Close the bleeder screw.
4. Repeat Step 3 until there are no air bubbles in the fluid.
5. Fill the reservoir with clutch fluid up to the proper level.