For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the front mud guard. Refer to Rear Mud Flap Guard Replacement .
4. Remove the engine protection shield. Refer to Engine Protection Shield Replacement .
5. Remove the screws and the front fender liner.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the screws and the front fender liner.

Tighten
Tighten the front fender liner screws to 4 N·m (35 lb in).

2. Install the engine protection shield. Refer to Engine Protection Shield Replacement .
3. Install the front mud guard. Refer to Rear Mud Flap Guard Replacement .
4. Install the front wheel. Refer to Tire and Wheel Removal and Installation .
5. Lower the vehicle.