For 1990-2009 cars

## Cigar Lighter Housing Replacement C100/Long Body

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the front console retainer.
3. Remove the front console cover trim panel.
4. Disconnect the electrical connectors.

### Installation Procedure

1. Install the front console cover in the gear lever cover.
2. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the front console retainer.

Tighten
Tighten the front console screws to 2 N·m (18 lb in).

4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .

## Cigar Lighter Housing Replacement C105/Short Body

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the rear floor console cover.
3. Remove the rear console cover trim panel.
4. Disconnect the electrical connectors.
5. Remove the screws and the cigar lighter housing.

### Installation Procedure

1. Install the cigar lighter housing with the screws.
2. Connect the electrical connector.
3. Install the rear console cover trim panel.
4. Install the rear console cover.
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .