For 1990-2009 cars

1. Install a new gasket (820) on the drain plug (819).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the drain plug (819) into the case assembly (17).

Tighten
Tighten the drain plug to 39 N·m (29 lb ft).

3. Install the vent hose assembly.
4. Install a new o-ring (824) on the transmission fluid level indicator and lubricate with transmission fluid.
5. Install the transmission fluid level indicator.
6. Install the transmission fluid level indicator bolt.

Tighten
Tighten the indicator bolt to 10 N·m (89 lb in).