For 1990-2009 cars

1. Measure the alignment on an alignment rack. Refer to Wheel Alignment Measurement.
2. Remove and discard the toe link-to-frame bolt, nut, and washer.

Note: Do not tighten the new fasteners yet in order to allow for movement.

3. Install a NEW cam washer to a NEW cam bolt.
4. Install the cam bolt with the washer to the toe link.
5. Install, but do not tighten, a NEW cam nut to the cam bolt.
6. Rotate the cam nut in order to adjust the toe angle. Refer to Wheel Alignment Specifications.
7. Hand tighten the cam bolt, but do not tighten the bolt to the specification yet.
8. Reinspect the rear toe angle and adjust as necessary.

Caution: Refer to Fastener Caution in the Preface section.

9. Hold the cam nut and tighten the cam bolt to 160 N·m (118 lb ft).
10. Repeat the procedure for the other rear wheel.
11. Lower the vehicle.