For 1990-2009 cars

### Removal Procedure

Important: Left - Hand Drive Shown, Right - Hand Drive Similar.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the screws at the base of the storage compartment.
3. Open and remove the screws.
4. Disconnect the electrical connector.
5. Remove the storage compartment.

### Installation Procedure

1. Position the storage compartment in the instrument panel.
2. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the storage compartment with the screws.

Tighten
Tighten the storage compartment screws to 2 N·m (18 lb in).

4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .