For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement.
3. Remove the screws and the door speaker.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the door speaker with the screws and tighten to 2 N·m (18 lb in).
3. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.