For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner Element Cover Screws | 2 N·m | 18 lb in
Air Cleaner Housing Bolts | 6 N·m | 53 lb in
Battery Hold-Down Bar Bracket Retaining Nuts | 10 N·m | 89 lb in
Battery Tray Retaining Bolts | 10 N·m | 89 lb in
Camshaft Bearing Cap Bolts | 8 N·m | 71 lb in
Connecting Rod Cap Bearing Bolts | 35 N·m plus 45° plus 15° | 26 lb ft plus 45° plus 15°
Coolant Bypass Housing Bolts | 15 N·m | 11 lb ft
Crankshaft Balancer Unit Assembly Bolts | 20 N·m plus 45° | 15 lb ft plus 45°
Crankshaft Bearing Cap Bolts | 50 N·m plus 45° plus 15° | 37 lb ft plus 45° plus 15°
Crankshaft Pulley Bolts | 20 N·m | 15 lb ft
Crankshaft Timing Belt Drive Gear Bolt | 135 N·m plus 30° plus 10° | 100 lb ft plus 30° plus 10°
Cylinder Head Bolts | 20 N·m plus 90° plus 90° plus 90° | 18 lb ft plus 90° plus 90° plus 90°
Cylinder Head Cover Bolts | 8 N·m | 71 lb in
Direct Ignition System and EGR Mounting Bracket Bolts | 25 N·m | 18 lb ft
Engine Beautification Cover Bolts and Nuts | 8 N·m | 71 lb in
Engine Beautification Cover Bracket Retaining Bolt | 20 N·m | 15 lb ft
Engine Fuse Block Lower Cover Bolts | 10 N·m | 89 lb in
Engine Fuse Block Retaining Bolts | 3 N·m | 27 lb in
Engine Mount Adapter Bolts | 50 N·m | 37 lb ft
Engine Mount Adapter Support Bracket Bolts | 45 N·m | 33 lb ft
Engine Mount Frame Side Bracket Bolt | 100 N·m | 74 lb ft
Engine Mount Frame Side Bracket Nuts | 90 N·m | 66 lb ft
Evaporative Emission Canister Purge Solenoid Bracket Bolt | 5 N·m | 44 lb in
Exhaust Camshaft Gear Bolt | 50 N·m plus 60° plus 15° | 37 lb ft plus 360° plus 15°
Exhaust Front Pipe Mounting Bracket Bolt and Nut | 40 N·m | 30 lb ft
Exhaust Manifold Heat Shield Bolts | 15 N·m | 11 lb ft
Exhaust Manifold Retaining Nuts | 22 N·m | 16 lb ft
Flexible Plate Bolts | 65 N·m | 48 lb ft
Flywheel Bolts | 65 N·m plus 30° plus 15° | 48 lb ft plus 30° plus 15°
Front Timing Belt Cover Bolts | 6 N·m | 53 lb in
Fuel Rail Assembly Retaining Bolts | 25 N·m | 18 lb ft
Generator-to-Generator Lower Support Bracket Through Bolt and Nut | 40 N·m | 30 lb ft
Generator-to-Intake Manifold Strap Bracket Bolt at Intake Manifold | 25 N·m | 18 lb ft
Generator-to-Intake Manifold Strap Bracket Bolt at Generator | 35 N·m | 26 lb ft
Generator Lower Support Bracket Bolts | 20 N·m | 18 lb ft
Generator Upper Brackets Bolts at Intake Manifold and Coolant Bypass Housing | 25 N·m | 18 lb ft
Generator Upper Bracket Bolt at Generator | 35 N·m | 26 lb ft
Intake Camshaft Gear Bolt | 50 N·m plus 60° plus 15° | 37 lb ft plus 60° plus 15°
Intake Manifold Retaining Bolt & Nuts | 18 N·m | 13 lb ft
Intake Manifold Support Bracket Bolt | 25 N·m | 18 lb ft
Interm Shaft Support Bracket Bolts | 70 N·m | 52 lb ft
Oil Filter Adapter-to-Oil Pump Bolts | 8 N·m | 71 lb in
Oil Pan Drain Plug | 18 N·m | 13 lb ft
Oil Pan Flange-to-Transaxle Retaining Bolts | 50 N·m | 37 lb ft
Oil Pan Retaining Bolts | 20 N·m | 15 lb ft
Oil Pressure Switch | 40 N·m | 30 lb ft
Oil Pump Rear Cover Bolts | 20 N·m | 15 lb ft
Oil Pump Retaining Bolts | 10 N·m | 89 lb in
Oil Suction Pipe Retaining Bolts | 8 N·m | 71 lb in
Pump Converter-to-Exhaust Front Pipe Retaining Nuts | 40 N·m | 30 lb ft
Rear Timing Belt Cover Bolts | 7 N·m | 62 lb in
Safety Relief Valve Bolt | 30 N·m | 22 lb ft
Spark Plugs | 25 N·m | 18 lb ft
Starter-to-Engine Block Mounting Bolt | 75 N·m | 55 lb ft
Starter-to-Transmission Mounting Bolt | 75 N·m | 55 lb ft
Timing Belt Automatic Tensioner Bolt | 25 N·m | 18 lb ft
Timing Belt Idler Pulley Bolt and Nut | 25 N·m | 18 lb ft
Transaxle Front Mount Retaining Bolts | 50 N·m | 37 lb ft
Transaxle Front Mount-to-Transaxle Through Bolt and Nut | 90 N·m | 66 lb ft
Transaxle Mount Assembly Retaining Bolts | 37 N·m | 27 lb ft
Transaxle Mount Bracket Retaining Bolts | 50 N·m | 37 lb ft
Transaxle Rear Mount Retaining Bolts | 90 N·m | 66 lb ft
Transaxle Rear Mount Bracket Retaining Bolts | 90 N·m | 66 lb ft
Transaxle Rear Mount-to-Bracket Through Bolt and Nut | 90 N·m | 66 lb ft
Transaxle-to-Oil Pan Flange Bolt | 50 N·m | 37 lb ft
Transaxle Torque Converter Bolts | 45 N·m | 33 lb ft