SMU - SECTION 6E2-A1 & 6E2-A2 DRIVEABILITY & EMISSIONS. Geo Metro 1996

For 1990-2009 cars

# SMU - SECTION 6E2-A1 & 6E2-A2 DRIVEABILITY & EMISSIONS

#### SUBJECT: SERVICE MANUAL UPDATE-SECTION 6E2-A1 AND 6E2-A2- DRIVEABILITY AND EMISSIONS-REVISED TABLE A1-1 AND A2-1 NO MALFUNCTION INDICATOR LAMP (MIL)

#### MODELS: 1996-97 GEO METRO WITH 1.0L AND 1.3L ENGINES (VINS 6, 9 - RPOS LP2, L72)

THIS BULLETIN IS BEING ISSUED TO REVISE THE DIAGNOSTIC TABLE A1-1 AND A2-1 NO MALFUNCTION INDICATOR LAMP (MIL) IN THE FOLLOWING SERVICE MANUALS:

GMP/96-M-2 AND GMP/97-M/2, SECTIONS 6E2-A1 AND 6E2-A2

THE ATTACHED REPLACEMENT PAGES SUPERSEDE THE DIAGNOSTIC TABLE ORIGINALLY PUBLISHED IN THE SERVICE MANUAL.

FIGURES: 00 ATTACHMENTS: 03

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.