SERVICE MANUAL UPDATE SEC. 6A MECHANICAL BEARING CHART REV.. Geo Metro 1991

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 6A MECHANICAL BEARING CHART REV.

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6 NE MECHANICAL - UNDERSIZED BEARING ART REPLACEMENT

#### VEHICLES AFFECTED: 1991 SPRINT/FIREFLY

Figure 1 in this bulletin replaces the chart in Figure 138 on page 6A1-42 of the 1991 Sprint/Firefly Service Manual (ST370-91). Refer to the table in Figure 1 for determining correct undersized bearing clearance.

#### MEASURED JOURNAL DIAMETER

44.744-44.750 mm 44.738-44.744 mm 44.732-44.738 mm (1.7616-1.7618") (1.7614-1.7616") (1.7612-1.7614")

LETTERS STAMPED A GREEN AND RED BLACK AND RED RED ONLY ON MATING SURFACE: B BLACK AND RED RED ONLY YELLOW AND RED C RED ONLY YELLOW A BLUE AND RED

UNDERSIZE BEARING TO BE INSTALLED

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.