SMU - SECTION 3A - WHEEL ALIGNMENT SPECIFICATION. Geo Metro 1992

For 1990-2009 cars

# SMU - SECTION 3A - WHEEL ALIGNMENT SPECIFICATION

********************************************************************** SERVICE MANUAL UPDATE **********************************************************************

#### SUBJECT: SECTION 3A - WHEEL ALIGNMENT SPECIFICATION

#### MODELS: 1990-94 GEO METRO

THE INFORMATION CONTAINED IN THIS BULLETIN AMENDS THE "TOE" ALIGNMENT SPECIFICATION (SECTION 3A) OF THE 1990-94 GEO METRO SERVICE MANUALS.

WHEN INSPECTING AND ADJUSTING TOE ALIGNMENT, USE THE SPECIFICATIONS SHOWN BELOW:

TOTAL TOE - FRONT - - - - - - - 0 +- .16 DEGREES TOTAL TOE - REAR - - - - - - - .16 +- .16 DEGREES

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.